|  |  |  |
| --- | --- | --- |
| BW CLIP SERIES SPECIFICATIONS |  |  |
| SIZE | 1.6 x 2.0 x 3.4 in. / 4.1 x 5.0 x 8.7 cm |  |
| WEIGHT | 3.2 oz. / 92 g |  |
| TEMPERATURES | BW Clip H2S:  BW Clip CO:  BW Clip O2 :  BW Clip SO2 : | -40 to +122°F / -40 to +50°C  -22 to +122°F / -30 to +50°C  -4 to +122°F / -20 to +50°C  -22 to +122°F / -30 to +50°C |
| HUMIDITY | 5% - 95% RH (non-condensing) |  |
| ALARMS | Visual, vibrating, audible (95 dB) • Low, High |  |
| TESTS | Activated detectors automatically perform one internal diagnostic test every 24 hours |  |
| TYPICAL BATTERY LIFE | Two years (H2S, CO, O2 or SO2 ) or three years (H2S or CO) depending on the version |  |
| EVENT LOGGING | 35 most recent events |  |
| INGRESS PROTECTION | IP 66/67 |  |
|  |  | Class I, Div. 1, Gr. A, B, C, D. |
|  |  | Class I, Zone 0 , Gr. IIC |
|  | ATEX: | II 1G Ex ia IIC T4 Ga |
| CERTIFICATIONS AND | IECEx: | Ex ia IIC T4 Ga |
| APPROVALS |  | European Conformity |
|  |  | American Bureau of Shipping |
|  |  | CU TR Ex (Customs Union) |
| WARRANTY | Two or three years from activation (given normal operation), plus one year shelf life (6 months for O2 ). Up to three years for two-year H2 S and CO detectors when used with the hibernation feature, limited to 24 months of detector operation. | |